|  |  |
| --- | --- |
| -Supply, grade and compact up to 50mm of granular A  -Heavy compaction at roadway and garage  -Supply and finish 50mm of SP12.5 Asphalt  -Caution tape and pickets at roadway when complete | $\_\_\_\_ .M2 |
| Supply Place and pack granular A additional to contract | $ \_\_\_\_\_ /mt |
| Ramps  Double | $ \_\_\_\_\_ ea |