|  |  |
| --- | --- |
| -Supply, grade and compact up to 50mm of granular A-Heavy compaction at roadway and garage-Supply and finish 50mm of SP12.5 Asphalt-Caution tape and pickets at roadway when complete | $\_\_\_\_ .M2 |
| Supply Place and pack granular A additional to contract | $ \_\_\_\_\_ /mt |
| RampsDouble | $ \_\_\_\_\_ ea |